CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.2.5/conf/instr/spect/uxnmr.info
Date         : Tue Jan 31 14:05:46 2017
Release      : TOPSPIN Version 3.2-pl5
Installed in : /opt/topspin3.2.5
Host         : dexter
OS           : CentOS release 5.5 (Final)
CPU          : Intel(R) Xeon(R) CPU W3505 @ 2.53GHz (2 cores at 1596 MHz)
User         : cclaudia (Claudia Cornilescu,,,,,,NMRFAM)
Description  : Avance III 600
Location     : NMRFAM, Univ. of Wisconsin - Madison
System       : Avance III NMR spectrometer
1H-frequency : 600.01 MHz
Order Number : 10022342
Configured in: /opt/topspin3.2.5/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.253
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU: AQS DRU-E Z102520/02102 ECL 06.01
- TCP/IP address = 149.236.99.89
- Firmware Version = 130419
- DRU controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x42   0x4    AW  R  4.4 REC-1  AQS RXAD600 Z102117/974 ECL 04.04
     3   0x34 0xc9   0x1        X  1.3 REF-1  REF/2-1000 Reference Board for AQS/2 Receiver
     4   0x24 0x19   0x8    AE  S  2.7 SGU-1  AQS SGU/2 600 Z103081/02398 ECL 02.07 FPGA-Vs=AF
     5   0x25 0x19   0x8    AE  S  2.7 SGU-2  AQS SGU/2 600 Z103081/02399 ECL 02.07 FPGA-Vs=AF
     6   0x26 0x19   0x8    AE  S  2.7 SGU-3  AQS SGU/2 600 Z103081/02400 ECL 02.07 FPGA-Vs=AF
     7   0x27 0x19   0x8    AE  S  2.7 SGU-4  AQS SGU/2 600 Z103081/02401 ECL 02.07 FPGA-Vs=AF
    21   0x21 0xcf     0        P  1.0 PSD-1  PSD/3 Power Supply Distribution Board
    --   0x20 0xd1     0        B  3.2 MASTER AQS/3 Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345094_0060 W1345094/0060 ECL 1:
- TCP/IP address = 149.236.99.252
- Firmware VS    = 20120627
- Amplifier      = BLA2X500 E 6-365MHZ INR: W1345094/0060 ECL 1
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/0971 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5047 ECL 50
BLA_W1345096_0638 W1345096/0638 ECL 2:
- TCP/IP address = 149.236.99.251
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H300/100/150 E 200-600MHZ INR: W1345096/0638 ECL 2
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/1023 ECL 0
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/5192 ECL 05
LTRX Z109890/00123 ECL 02.00:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00123 ECL 02.00

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20150423
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 600: Z109890/00123 ECL 02.00
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB-E SENSOR & PNEUMATIC BD: Z115192/00051 ECL 02.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/00179 ECL 01.01

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Bruker Automatic Changer: device connected to 149.236.99.253:/dev/tty04
- Capacity: 596 holders
- Firmware: 970111
- use BACS air  = yes
- BACS sx delay = 10 s
- Sample Rail fast changer mode = no

Sample Changers at the spectrometer subnet:
-------------------------------------------
 - SampleJet: at TCP/IP address 149.236.99.55


Cryo Controller CRCO: device connected to 149.236.99.253:/dev/tty05

Preamplifiers :
HPPR: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Application firmware = AQ
                15 LEDs for tuning, 15 LEDs for matching
    Module  1 : 1H LNA
                 PN=Z003462, SN=00765 from 20100827
    Module  2 : XBB19F 2HS
                 PN=Z003506, SN=00899 from 20101001
    Module  3 : 2H
                 PN=Z003473, SN=00773 from 20100818
    Module  4 : 13C
                 PN=Z003524, SN=00494 from 20100824
    Module  5 : 15N
                 PN=Z003530, SN=00387 from 20100927
    Module  6 : 31P
                 PN=Z102449, SN=00017 from 20091219


Frequency generation:
- F1: for SGU
- F2: for SGU
- F3: for SGU
- F4: for SGU



RF cable connections (detected by 'confamp')
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0638 at TCP/IP 149.236.99.251)
SGU1 AUX  output -> input 1 of transmitter 1 (BLA2X500 E 6-365MHZ INR W1345094/0060 at TCP/IP 149.236.99.252)
SGU2 NORM output -> input 2 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0638 at TCP/IP 149.236.99.251)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 3 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0638 at TCP/IP 149.236.99.251)
SGU3 AUX  output -> input 2 of transmitter 1 (BLA2X500 E 6-365MHZ INR W1345094/0060 at TCP/IP 149.236.99.252)
SGU4 NORM output -> input 3 of transmitter 1 (BLA2X500 E 6-365MHZ INR W1345094/0060 at TCP/IP 149.236.99.252)
SGU4 AUX  output -> input 4 of transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0638 at TCP/IP 149.236.99.251)

Blanking cable connections (detected by 'confamp')
--------------------------------------------------------------------
transmitter 1 (BLA2X500 E 6-365MHZ INR W1345094/0060 at TCP/IP 149.236.99.252) amplifier X-500W uses blanking 3
transmitter 1 (BLA2X500 E 6-365MHZ INR W1345094/0060 at TCP/IP 149.236.99.252) amplifier X-500W uses blanking 4
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0638 at TCP/IP 149.236.99.251) amplifier 1H-100W uses blanking 2
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0638 at TCP/IP 149.236.99.251) amplifier X-300W uses blanking 1
transmitter 2 (BLAXH2H300/100/150 E 200-600MHZ W1345096/0638 at TCP/IP 149.236.99.251) amplifier 2H-150W needs no blanking
transmitter 3 (BSMS/2 LOCK TRANSCEIVER 600 Z109890/00123 at TCP/IP 149.236.99.20) amplifier 2H-5W needs no blanking

