CONFIGURATION INFORMATION
=========================

Path         : /opt/topspin3.5pl5/conf/instr/spect/uxnmr.info
Date         : Wed Aug 10 09:43:23 2016
Release      : TopSpin 3.5 pl 5
Installed in : /opt/topspin3.5pl5
Host         : fleckvieh
OS           : CentOS Linux release 7.2.1511 (Core) 
CPU          : Intel(R) Xeon(R) CPU E5-1620 v3 @ 3.50GHz (8 cores at 1300 MHz with Hyperthreading)
User         : nmrsu (NMR SuperUser)
System       : Avance III HD 900 NMR spectrometer
1H-frequency : 899.75 MHz
Description  : AVHD900X
Configured in: fleckvieh:/opt/topspin3.5pl5/conf/instr/spect

IPSO: connected to spectrometer subnet
- TCP/IP address = 149.236.99.90
 - IPSO type: 19"
- Tctrl : 1
- Fctrls: 4
- Gctrl1: without digital preemphasis
- Rctrl : none
- FREDs : none
- DPP : none

DRU1: AQS DRU-E Z102520/05043 ECL 07.00
- TCP/IP address = 149.236.99.89
- Firmware Version = 151014
- DRU1 controls AQS-Rack and HPPR/2

AQS: connected to 149.236.99.89:/dev/tty10
  _Slot_ SBSB _____________________Board_____________________
  Number Addr Type HW-VS FW-VS ID  ECL Name   Description
  -----------------------------------------------------------
     2   0x10 0x53   0x5    CD  R  0.3 REC-1  AQS RXAD/2 1000 Z130589/415 ECL 00.03
     3   0x34 0xda   0x1        X  2.3 REF-1  
     4   0x24 0x33     0        S  1.3 SGU-1  AQS SGU/3 1200 (2CH) Z117130/00623 ECL 01.03 FPGA-Vs=20131031
     5   0x26 0x33     0        S  1.3 SGU-2  AQS SGU/3 1200 (2CH) Z117130/00624 ECL 01.03 FPGA-Vs=20131031
    13   0xa0 0x93     0        V  0.1 PS-1   
    14   0xa1 0x91     0        V  1.2 PS-2   AQS PSM-D Power Supply Module
    --   0x20 0xd8     0        B  2.0 MASTER AQS/3+ Chassis
     1   0x20  0x7     0        B      MASTER AQS Rack Master
  Logical Receiver/SGU configuration:


Router: none installed


Transmitters at the spectrometer subnet:
----------------------------------------
BLA_W1345528_0009 W1345528/0009 ECL 20:
- TCP/IP address = 149.236.99.95
- Firmware VS    = 20120627
- Amplifier      = BLAH500 E 700-900MHZ INR OUTR: W1345528/0009 ECL 20
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/5235 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011294 ECL 60
BLA_W1345529_0234 W1345529/0234 ECL 01:
- TCP/IP address = 149.236.99.93
- Firmware VS    = 20120627
- Amplifier      = BLAX1000 E 6-405MHZ INR OUTR: W1345529/0234 ECL 01
- Router         = BLMMR31 RF AMPLIFIER MODULE: W1345212/005252 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/011155 ECL 60
BLA_W1345097_0390 W1345097/0390 ECL 20:
- TCP/IP address = 149.236.99.91
- Firmware VS    = 20120627
- Amplifier      = BLAXH2H500/100/250 E 700-900MHZ INR: W1345097/0390 ECL 20
- Router         = BLMMR32 RF AMPLIFIER MODULE: W1345204/5302 ECL 21
- Controller     = BLA CONTROL BOARD 6 2CH: W1522050/11141 ECL 60
LTRX Z109895/00202 ECL 01.01:
- TCP/IP address = 149.236.99.20
- Amplifier      = BSMS/2 LOCK TRANSCEIVER 900: Z109895/00202 ECL 01.01

BSMS: BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20
- ELCB firmware version = 20150423
- GAB current limits = 0.0/X, 0.0/Y, 10.0/Z (in A)
- SCB channels = 40
- Shim System = BOSS3-SB
- L-TRX = BSMS/2 LOCK TRANSCEIVER 900: Z109895/00202 ECL 01.01
- Lock: on L-TRX board
- VTU_SPB = BSMS/2 SPB SENSOR & PNEUMATIC BD: Z115191/03138 ECL 04.00
- VTU_VPSB1 = BSMS/2 VARIABLE POWER SUPPLY BD: Z115193/03456 ECL 01.05

VTU: in BSMS/2 connected to ethernet
- TCP/IP address = 149.236.99.20

Cryo Controller CRCO: device connected to 149.236.99.90:/dev/tty04

Preamplifiers :
HPPR2: - HPPR/2 preamplifier connected to 149.236.99.89:/dev/tty10
    Type      : HPPR/2
    Controller: Cover/2, with DRU Application firmware = c.
                no LED display for tuning and matching
    Module  1 : HPLNA 19F1H (virtual 50 Ohm reference: 101.1%/-0.3deg, reflection meter)
                PN=Z103209, SN=00204 from 20160125
    Module  2 : HPLNA 19F1H (virtual 50 Ohm reference: 101.1%/-0.1deg, reflection meter)
                PN=Z103209, SN=00203 from 20160125
    Module  3 : 2H
                PN=Z003477, SN=00203 from 20150120
    Module  4 : 13C
                PN=Z003528, SN=00202 from 20150121
    Module  5 : 15N
                PN=Z003534, SN=00201 from 20150120
    Module  6 : HPLNA BB31P (reflection meter)
                PN=Z111098, SN=00206 from 20160126
    Module  7 : HPLNA BB31P (reflection meter)
                PN=Z111098, SN=00205 from 20150915



Gradient Controller cable connections
--------------------------------------------------------------------
GCtrl1: connected to GAB in BSMS

RF cable connections (detected)
--------------------------------------------------------------------
SGU1 NORM output -> input 1 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 900 W1345097/0390 at TCP/IP 149.236.99.91)
SGU1 AUX  output -> input 2 of transmitter 2 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0234 at TCP/IP 149.236.99.93)
SGU2 NORM output -> input 2 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 900 W1345097/0390 at TCP/IP 149.236.99.91)
SGU2 AUX  output -> TUNE signal input of HPPR
SGU3 NORM output -> input 1 of transmitter 2 (BLAX1000 E 6-405MHZ INR OUTR W1345529/0234 at TCP/IP 149.236.99.93)
SGU3 AUX  output -> input 3 of transmitter 1 (BLAH500 E 700-900MHZ INR OUTR W1345528/0009 at TCP/IP 149.236.99.95)
SGU4 NORM output -> input 2 of transmitter 1 (BLAH500 E 700-900MHZ INR OUTR W1345528/0009 at TCP/IP 149.236.99.95)
SGU4 AUX  output -> input 4 of transmitter 3 (BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 900 W1345097/0390 at TCP/IP 149.236.99.91)

Blanking cable connections (detected)
--------------------------------------------------------------------
transmitter 1 = BLAH500 E 700-900MHZ INR OUTR W1345528/0009 at TCP/IP 149.236.99.95:
- amplifier 1H-500W uses blanking 4
- amplifier 1H-50W uses blanking 4

transmitter 2 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0234 at TCP/IP 149.236.99.93:
- amplifier X-1000W uses blanking 3
- amplifier X-300W uses blanking 3

transmitter 3 = BLAXH2H500/100/250 E 700-900MHZ BSMS/2 LOCK TRANSCEIVER 900 W1345097/0390 at TCP/IP 149.236.99.91:
- amplifier 1H-100W uses blanking 2
- amplifier X-500W uses blanking 1
- amplifier 2H-250W uses blanking 7

transmitter 4 = BSMS/2 LOCK TRANSCEIVER 900 Z109895/00202 at TCP/IP 149.236.99.20:
- amplifier 2H-5W needs no blanking


Switchbox (unknown: no outputs) routing
--------------------------------------------------------------------
transmitter 1 = BLAH500 E 700-900MHZ INR OUTR W1345528/0009 at TCP/IP 149.236.99.95:
- amplifier 1H-500W at blanking 4 can be routed to switchbox output 1 (unknown) and output 2 (unknown)

transmitter 2 = BLAX1000 E 6-405MHZ INR OUTR W1345529/0234 at TCP/IP 149.236.99.93:
- amplifier X-1000W at blanking 3 can be routed to switchbox output 1 (unknown) and output 2 (unknown)


